**Comandos de Configuração pra IP ESTÁTICO**

enable

conf t

hostname NOME DO SWITCH

vlan 2

name vlan2

exit

interface vlan 1

ip address ENDEREÇO DE IP MÁSCARA DE REDE

no shutdown

exit

interface vlan 2

ip address ENDEREÇO DE IP MÁSCARA DE REDE

exit

interface gigabitEthernet 0/1

switchport mode trunk

switchport trunk allowed vlan all

exit

interface gigabitEthernet 0/2

switchport mode trunk

switchport trunk allowed vlan all

exit

interface range fastEthernet 0/1 - fastEthernet 0/12

switchport mode access

switchport access vlan 1

exit

interface range fastEthernet 0/13 - fastEthernet 0/24

switchport mode access

switchport access vlan 2

exit

exit

wr

copy running-config startup-config

exit

**Comandos de Configuração pra IP DINÃMICO**

enable

conf t

hostname NOME DO SWITCH

vlan 2

name vlan2

exit

interface vlan 1

ip address ENDEREÇO DE IP MÁSCARA DE REDE

no shutdown

exit

interface vlan 2

ip address ENDEREÇO DE IP MÁSCARA DE REDE

exit

interface gigabitEthernet 0/1

switchport mode trunk

switchport trunk allowed vlan all

exit

interface gigabitEthernet 0/2

switchport mode trunk

switchport trunk allowed vlan all

exit

interface range fastEthernet 0/1 - fastEthernet 0/12

switchport mode access

switchport access vlan 1

exit

interface range fastEthernet 0/13 - fastEthernet 0/24

switchport mode access

switchport access vlan 2

exit

ip dhcp pool AcessosCompras

network ENDEREÇO DE REDE MÁSCARA DE REDE

default-router ENDEREÇO DE BROADCAST

exit

exit

wr

copy running-config startup-config

exit